Scaling in OpenSim:

1. Use the static trail markerdata to scale the generic model.
2. Scale model:
3. Without setup file -> Adjust model markers -> your static.trc
4. With setup file -> Load -> Setup file -> name your scaled model & enter bodyweight.
5. Check scale factors
6. Check static pose weights